Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 156 - 2615_KEC
P. 156

    4.  Circuit Setup:

                              Connect the Servo Motors:
                              o   Connect the continuous servo motors to the GPIO pins on the Micro:bit.

                              o  Secure the servo motors and wheels to the readymade chassis.

                              o  Ensure that the wiring is secure and the motors are properly mounted.
                      5.  Testing the Setup:

                              After assembling the car and uploading the code to the Micro:bit, test the car:
                              o  ‘f’: Car should move forward.

                              o  ‘b’: Car should move backward.

                              o  ‘l’: Car should turn left.
                              o  ‘r’: Car should turn right.

                              o  ‘s’: Car should stop.

                      6.  Final Testing and Adjustments:
                              Check for stable Bluetooth connectivity.

                              Ensure the servo motors respond accurately to the commands, making any necessary
                              adjustments to the motor speeds for smoother operation.

                      Download link of Bluetooth App-
                      https://play.google.com/store/apps/details?id=com.ev_developers.ev_microbit&hl=en_IN&pli=1

                      154   Premium Edition-VI

| 151 152 153 154 155 156 157 158 159 160 161 |