Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 112 - 2629_Devagiri_C-8
P. 112

    TYPES OF VIRTUAL ROBOTS
                      Depending on their tasks and where they are used, virtual robots can be divided into several

                      types. The different types of virtual robots are as follows:
                          Educational  robots: Used  in  schools  and  online  platforms  to
                         teach coding and robotics.

                                                       Simulation robots: Help scientists and engineers test machines
                                                      before building real ones.

                          Entertainment robots: Used in games or apps to provide fun and
                         interactive experiences.

                      SENSORS IN VIRTUAL ROBOTS

                      Virtual robots can be equipped with various types of sensors to interact with their environment.
                      These sensors are designed to simulate real-world perception, similar to those used in physical
                      robots. Some common types of sensors in virtual robots are as follows:
                          Distance sensor: Measures the distance between the robot and objects in its path. It helps
                         the robot avoid obstacles or navigate through spaces.
                          Gyro sensor: Measures the robot’s  rotation and orientation.  It helps the robot  stay
                         balanced or turn to a specific angle.

                          Encoder: Measures the rotation of the wheels or motors to help the robot track its movements
                         and distance travelled.
                          Eye sensor: Helps the robot see and process visual information.

                         •  Front Eye sensor: Detects objects and their colours in front of the robot. It also acts as a
                            distance sensor, reporting the distance to an object in millimetres or inches.
                         •  Down Eye sensor: Points downward and can detect the colour of the surface below the robot.
                          Bumper  sensor: Detects  physical  contact  with objects.  It helps robot  to avoid  obstacles,
                         prevent collisions or trigger certain actions when they hit or touch something.
                          Location sensor: Reports the robot’s (X, Y) coordinate position and heading angle, enabling
                         precise tracking of the robot’s location on the virtual playground.

                             GETTING STARTED WITH VEXCODE VR

                      VEXcode VR is an online platform that allows you to learn robotics and programming using virtual
                      robots, without requiring any physical hardware. With just a computer and an Internet connection,
                      you can program virtual robots to move, turn, draw and solve puzzles. The platform uses intuitive
                      block-based coding, making it easy for beginners to get started.

                       110
                            Premium Edition-VIII

| 107 108 109 110 111 112 113 114 115 116 117 |