Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 166 - CodePilot V5.0 C7
P. 166

    To turn on an LED using a breadboard, follow the given steps:

                       Step  1    Open your web browser, type https://www.tinkercad.com and press Enter key.
                       Step  2    Log in to your Tinkercad account.

                       Step  3     Click on the Create button and select Circuits from the dropdown menu.

                      A new circuit design workspace will open.
                      Now, recreate the circuit by dragging the components (LED, Coin Battery, Breadboard, Resistor)

                      from the components library and placing them on the breadboard.
                       Step  4    Click on the Project Name and rename your project (Circuit).

                       Step  5    Connect the positive terminal of the coin battery to the breadboard’s positive rail.

                       Step  6    Connect the negative terminal of the coin battery to the breadboard’s negative rail.

                       Step  7    Connect the resistor to the battery’s positive terminal and the LED’s anode.

                       Step  8    Connect the LED’s cathode to the negative rail.

                       Step  9    Click on Start Simulation to test the circuit.

                                                                                                  SHORT SIGN

                                                                                                  To insert a note: N

                      The output  shows the  LED lighting  up,  indicating  that  the  circuit  is  correctly  connected  and
                      functioning as expected.

                       164
                            CodePilot (V5.0)-VII

| 161 162 163 164 165 166 167 168 169 170 171 |