Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 23 - RoboGenius Pro C5
P. 23

    Difference Between Hardware and Virtual Components

                     Hardware and virtual components work together to make a robot functional, but

                     they serve different purposes and exist in different forms. Some of the key differences
                     between hardware and virtual components are as follows:

                          Key             Hardware Components                         Virtual Components
                      Difference

                      Nature          Tangible and visible.                   Invisible, software-based.

                      Function        Interact with the physical world  Control actions,  make decisions,

                                      (movement, sensing).                    process data.

                      Change          Hard to change once built.              Easy to edit or update.

                      Testing         Needs real tools and space.             Tested safely through simulations.

                      Example         Motors, wheels, sensors, arms,  Control system, AI, programming,
                                      body, etc.                              simulation tools, etc.

                     SIMULATION BENEFITS AND LIMITATIONS

                     Simulation  allows us  to  test  and  design  robots  in  a  virtual  environment  before

                     building them in the real world. While it offers many advantages, there are also
                     some limitations to keep in mind.

                     Benefits of Simulation

                     Simulation offers many benefits that make learning and building robots easier and
                     safer. Some of its major benefits are:

                        n Reduces risk: Simulation lets us test robots safely on a computer, helping us find
                        and fix problems without damaging real parts.

                        n Reduces costs: It helps save money by testing designs virtually, reducing the
                        need for physical prototypes.

                        n Saves time: It speeds up the development process by allowing multiple tests and

                        adjustments in a short amount of time.

                        n Safety: Potential risks can be tested in a virtual environment without putting
                        people or expensive equipment in danger.

                        n Efficient problem solving:  Errors and issues can be identified early, making it
                        easier to fix problems before building the physical robot.

                                                                         Exploring Real vs Simulated Components
                                                                                                                        21

| 18 19 20 21 22 23 24 25 26 27 28 |