Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 36 - RoboGenius Pro C5
P. 36

    Connections

                      To connect the buzzer, use the pins at the bottom edge of the Micro:bit:

                         n Connect the positive (+) wire of the buzzer to Pin 0 (Pin-0).

                         n Connect the negative (–) wire of the buzzer to the GND pin.

                      These connections allow the Micro:bit to send signals through the pins that make

                      the buzzer produce sound. Follow the given steps to create the buzzer project:

                        STEP - 1   Visit the link: https://makecode.microbit.org/ or scan the
                                     QR code.

                        STEP - 2   Click on the New Project option.

                        STEP - 3   Type the project name Buzzer in the Create a Project window and click
                                     on the Create button.

                                                           Buzzer

                                     The Micro:bit editor window will appear.

                                     RoboGenius Pro - V
                     34

| 31 32 33 34 35 36 37 38 39 40 41 |