Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 49 - RoboGenius Pro C7
P. 49

    Code: Displays the blocks that control the robot’s actions in the simulation, with the when
                        started block appearing by default.

                        SELECT PLAYGROUND: A button to choose the virtual environment (playground) where the
                        robot performs its actions.
                        OPEN PLAYGROUND: Opens the selected playground to start the robot’s simulation.

                         Simulation Controls: Includes START, STEP and STOP buttons to control the simulation of the
                        robot.
                        Code  Viewer: Displays  the  created  code  in a  readable,  structured  format,  showing  the
                        sequence of the code.

                        Monitor: Shows the area where outputs from the code are displayed during the simulation.
                        File Menu: Manages projects with options like New, Open, Save, Save As and more.

                        UNDO/REDO: The UNDO button reverts the last action and REDO restores the undone action.

                            VISUAL VAULT
                            Identify the following components of VEXcode VR:

                            1.                                                2.

                            3.                                                4.

                     THE VEX VR ROBOT

                     The VEX VR Robot is a virtual robot that students can program within
                     the VEXcode VR platform. It performs all the actions of a real robot such
                     as moving, turning, sensing and drawing within a simulated environment
                     called a Playground.

                     VEX VR Robot Built-in Features

                     The VEX VR Robot comes with several built-in parts that help it sense, move and interact within
                     the virtual playground.

                                                                                                  Built-in Gyro +
                               Pen                                                                Location Sensing

                         Electromagnet

                                      Down Eye                                                    Left Bumper Sensor

                               50 mm Diameter Wheels        Right Bumper Sensor      Front Eye + Distance Sensor

                                                                               Getting Started with VEXcode VR
                                                                                                                        47

| 44 45 46 47 48 49 50 51 52 53 54 |