Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 54 - RoboGenius Pro C8
P. 54

    STEP - 4   Click on the Mic button inside the default Background Noise class. This teaches the
                                   model what silence or normal background sound is.

                       STEP - 5   Click on the Record 20 Seconds button to record background noise. You can also
                                   change the duration by clicking on the Setting button.

                       STEP - 6   After  completing  the  recording,  click  on the  Extract  Sample button  to  add
                                   audio samples.

                                   Similarly, add audio samples to class Whistle and Clap.

                                     RoboGenius Pro - VIII
                     52

| 49 50 51 52 53 54 55 56 57 58 59 |