Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 42 - Robo_Genius_V1.0_flipbook_C4
P. 42

    Battery                       2 Jumper wire                  Battery OTG Socket

                                    Magnetic Board                      USB Cable

                      Step 2  Put the LED module on the Magnetic board.

                      Step 3  After LED connect the resistor to the negative terminal of the LED.

                      Step 4  Connect switch to the resistor and then, connect the battery.

                      Step 5  The  Positive  terminal  of  the  battery  is  connected  to  the  positive
                                 terminal  of  the  LED  and  the  negative  terminal  of  the  battery  is
                                 connected to the switch.

                      Step 6  See the result.

                          40     RoboGenius (V1.0)-IV

| 37 38 39 40 41 42 43 44 45 46 47 |