Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 76 - Robo_Genius_V1.0_flipbook_C4
P. 76

    and measure the surrounding light levels. This dual function lets the micro:bit
                      respond  dynamically  to  different  lighting
                                                                                        START
                      conditions.
                                                                                        FOREVER
                      Algorithm Used                                                        READ THE LIGHT VALUE

                                                                                            IF MORE THAN 100
                      An algorithm is a step-by-step procedure that
                                                                                            TURN LEDS ON
                      defines  a  set  of  instructions  that  must  be                     ELSE

                      carried out in a specific order to produce the                        CLEAR SCREEN
                      desired result.                                                   END

                                                                                                             21 st   #Creativity
                        Activity       Programming a Sunlight Sensor                                       Century
                                                                                                             Skills
                                       Using Micro:bit

                      Step 1  Go to Microsoft make code https://makecode.microbit.org/

                      Step 2  Click on new projects.

                                            Click on new
                                            project

                      Step 3   Create a project.

                                                                   Create a project

                           74    RoboGenius (V1.0)-IV

| 71 72 73 74 75 76 77 78 79 80 81 |