Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 19 - Robo_Genius_V1.0_flipbook_C7
P. 19

    Step 4  Connect the positive terminal of the battery to the input
                              terminal of the 7805 voltage regulator IC.
                     Step 5  Connect  the  ground  terminal  of the  7805 IC  to  the
                              negative terminal of the battery.

                                                     Step 6   Connect the output terminal of the 7805 IC (+5V) to the
                                                              positive rail of the breadboard.

                     Step 7  Place the LED on the breadboard.

                     Step 8  Place a resistor on the breadboard as shown in the image.

                                                     Short Lead    Step 9   Connect  the  shorter  lead  (cathode)  of  the
                                                     (Cathode)
                                                                            LED to the ground terminal of the 7805 IC.

                                                                                                              Longer Lead
                                                                                                                (Anode)

                     Step 10  Now, connect the longer lead (anode) of the LED to the
                              second end of the resistor as shown in the image.

                                                                   Hands-On Electronics with Breadboard-Based Kit  17

| 14 15 16 17 18 19 20 21 22 23 24 |