Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 22 - Robo_Genius_V1.0_flipbook_C7
P. 22

    Circuit Diagram

                      Circuit Setup Steps

                      Step 1  Take a breadboard.
                      Step 2  Connect the 7805 voltage regulator IC to the breadboard as shown.

                      Step 3  Take a battery and connect the battery cap.

                                                       Step 4   Connect the positive terminal of the battery to the input
                                                                terminal of the 7805 voltage regulator IC.

                                                       Step 5   Connect the ground terminal of the 7805 IC to the negative
                                                                terminal of the battery.

                      Step 6  Connect the output terminal of the 7805 IC (+5V) to the
                               positive rail of the breadboard.

                                                       Step 7  Place the LED on breadboard.
                                                       Step 8   Connect the ground terminal of the 7805 IC to the negative
                                                                rail of the breadboard.

                          20     RoboGenius (V1.0)-VII

| 17 18 19 20 21 22 23 24 25 26 27 |