Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 67 - Robo_Genius_V1.0_flipbook_C7
P. 67

    Step 4  Place the 12T gear on the motor shaft, then install the spacer and
                              axle lock as shown in the image.

                              Connect the 60T gear using axel lock and a small shaft as shown
                              the image.
                                              Connect  a  small  “L” plate  on  60T  gear  using  a
                                              small bolt and nut as shown in the image.

                                              Attach the motor to the motor shaft
                                              and secure it on the small ‘L’ bracket
                                              using  the  screw  provided  with  the
                                              motor. Place the shaft locker on the
                                              motor shaft as shown.

                                              Connect the two small bars using nuts
                                              and small bolts.

                     Finally, connect a hook as shown in the image.
                     Step 5  Connect the motor’s wire to the power distribution
                              board, connect the power distribution board to the remote using a data cable, Now, plug
                              the adapter into the socket and connect it with the remote to power the Robo Crane.

                     Concepts

                      Understanding Motion: Exploring concepts of movement, speed, and direction as they relate to
                       the crane’s arm and hook.

                      Forces and Stability: Discussing the forces acting on the crane, including gravity and balance
                       when lifting different loads.

                                                                          Mechanical Concepts with Mechatron Kit  65

| 62 63 64 65 66 67 68 69 70 71 72 |