Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 26 - Robo_Genius_V1.0_flipbook_C7
P. 26

    Circuit Diagram

                      Circuit Setup Steps

                      Step 1  Take a breadboard.

                      Step 2  Connect the 7805 voltage regulator IC to the breadboard as shown.

                      Step 3  Take a battery and connect the battery cap.

                                                   Step 4   Connect  the  positive  terminal  of  the  battery  to  the  input
                                                            terminal of the 7805 voltage regulator IC.

                                                   Step 5   Connect the ground terminal of the 7805 IC to the negative
                                                            terminal of the battery.

                      Step 6  Connect the output terminal of the 7805 IC (+5V) to the
                               positive rail of the breadboard.

                                                                                 Step 7   Connect the ground terminal of
                                                                                          the 7805 IC (0V) to the negative
                                                                                          rail of the breadboard.

                                                                                 Step 8   Insert  an  NPN  transistor  and
                                                                                          LDR sensor into the breadboard.

                           24    RoboGenius (V1.0)-VII

| 21 22 23 24 25 26 27 28 29 30 31 |