Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 48 - Robo_Genius_V1.0_flipbook_C7
P. 48

    Step 4  Click on Sensors option and drag Read IR on block and drop inside first blank space of
                               comparison operator and change the pin AO. Click on math option, drag number block and
                               drop it inside a second blank space of comparison operator and change the value from
                               accordingly. Also change the comparison (=) operator into less than (<) operator.

                      Step 5  Click on setting option given on if block, add else with if.

                      Step 6  Click on OUTPUT option, drag block Set MOTOR on and HIGH, drop it inside a if condition
                               and change pin 0 to pin 6. Similarly drag Set MOTOR on block again from the output, change
                               the pin number to 6 and attach it with logic LOW inside a else condition.

                           46    RoboGenius (V1.0)-VII

| 43 44 45 46 47 48 49 50 51 52 53 |