Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 182 - 2615_KEC
P. 182

    To extrude, follow these steps:

                      Step  1  In the top-left corner of the 3D Viewport, click on the Mode drop-down menu.
                      Step  2  Choose Edit Mode from the drop-down list.

                      Step  3  Select Vertex, Edge or Face Mode.

                      Step  4  Click on a vertex, edge or face to select it.
                      Step  5  Click on the Extrude Region Tool from the Toolbar.

                              OR

                              Press E on the keyboard.
                      Step  6  Move the mouse to extend the selection.

                      Step  7  Click to confirm the extrusion.

                      LOOP CUT

                      Loop Cuts add new edges to an object, helping refine shapes for smoother models. It’s useful for
                      adding details in objects like buildings, characters and mechanical parts.
                      To use Loop Cut tool, follow these steps:

                      Step  1  Select the object you want to modify.
                      Step  2  Switch to Edit Mode by clicking the
                      Mode drop-down menu.

                              OR
                              Press Tab on the keyboard.

                      Step  3   Click on the Loop Cut Tool from the
                              Toolbar on the left.
                              OR

                                Press  Ctrl  + R on the keyboard  to
                              activate the Loop Cut Tool.

                      180   Premium Edition-VII

| 177 178 179 180 181 182 183 184 185 186 187 |