Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 128 - 2629_Devagiri_C-8
P. 128

    The explanation of the code is as follows:
                          The program starts when the when started block is triggered.

                          The robot’s drive and turn velocity is set to 100% for full speed.
                          A while loop runs until the Down Eye sensor detects red beneath the robot and checks the distance:

                         •  If the distance is greater than 200 mm, it drives 250 mm forward, then turns right by 90°.
                         •  If the distance is less than 200 mm, it turns left by 90° to find a clear path.

                          Once red is detected, the loop ends and the robot stops.

                       RAPID RECALL                             Tick ( ) if you know this.

                          1.  Control blocks let you decide when and how often the robot acts.

                          2.  Distance sensing blocks use the robot’s distance sensor to measure the space
                              between the  robot and obstacles.

                                                                                                 21 st   #Critical Thinking
                           EXPERIENTIAL LEARNING                                                Century   #Technology Literacy
                                                                                                 Skills
                        Draw geometric shapes like squares, triangles and hexagon using Drawing blocks.

                             USING MAGNET BLOCKS

                      Magnet  blocks allow the  virtual robot  to  pick  up  and drop  magnetic  disks  using  its  built-in
                      electromagnet. These blocks are essential for simulations where the robot interacts with objects
                      like coloured disks.

                                                          energize Magnet   to  boost

                      The Magnet Block in VEXcode VR has two settings:
                          Boost: This increases the magnet’s strength so the robot can pick up multiple disks at once. It
                         is useful when you need to collect a group of disks quickly.

                          Drop: This lowers the strength of the magnet so it can release the disks it is carrying. The robot
                         drops them at the desired location (like a goal zone).

                        Program 7 Prepare a disk mover program.

                      The  robot’s  task  is to  locate,  pick  up and sort coloured  disks  on the Disk Mover playground.
                      Using its electromagnet and sensor logic, it must identify each disk’s colour and transport it to

                      the corresponding drop zone.

                       126
                            Premium Edition-VIII

| 123 124 125 126 127 128 129 130 131 132 133 |