Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 121 - 2629_Devagiri_C-8
P. 121

    In the above code, the blocks are repeated four times.
                     Instead of repeating the same block multiple times, the repeat block can be used. It allows for the

                     efficient execution of a sequence of commands multiple times, making programs more concise
                     and powerful.
                     Now, to move the robot on the Grid Map playground in a
                     zig-zag pattern, use the repeat block.                           when started

                     The explanation of the given code is as follows:
                                                                                       repeat  4
                         The  program  starts  when the  when started  block  is
                        triggered.                                                      turn  right  for  60  degrees
                         The robot first turns right by 60 degrees.                     drive  forward  for  200  mm

                         Then, it drives forward for 200 mm.                            turn  left  for  60  degrees
                         It turns left by 60 degrees and drives forward for 200 mm.
                                                                                        drive  forward  for  200  mm
                         This  process  repeats 4 times,  with the  robot  making
                        small adjustments to create a square-like path.

                      Program 2 Move the robot to the centre of the Grid Map playground in circular pattern.

                     The task is to make the robot move in a circular pattern starting from the centre of the Grid Map
                     playground. The code and output of the given task is as follows:

                       when started

                       turn  right  for  90  degrees

                       drive  forward  for  575  mm

                       turn  left  for  90  degrees

                       drive  forward  for  875  mm

                       repeat  36

                        drive  forward  for  60  mm

                        turn  right  for  10  degrees

                     The explanation of the given code is as follows:
                         The program starts when the when started block is triggered.

                         The robot first turns 90 degrees.
                         Then, it drives forward 575 mm.

                         It turns left by 90 degrees and drives forward 875 mm.

                                                                                                                      119
                                                                                     VEXcode VR: Drive, Sense and Create

| 116 117 118 119 120 121 122 123 124 125 126 |