Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 41 - RoboGenius Pro C4
P. 41

    STEP - 6   Drag the pause (ms) block from the Basic block category and place it

                                     after the show icon block. Set the value to 1000 ms (1 second), which
                                     will make the icon display for 1 second.

                      STEP - 7   Drag the clear screen block from the Basic block category and place

                                     it after the pause (ms) block. This block will clear the icon displayed on
                                     the screen.

                      STEP - 8   Drag the pause (ms) block from the Basic block category and place

                                     it after the clear screen block. Set the value to 500 ms (0.5 seconds).
                                     This will create a half-second pause before the next iteration of the
                                     loop begins.

                                                                                         Coding with Micro:Bit
                                                                                                                        39

| 36 37 38 39 40 41 42 43 44 45 46 |