Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 34 - RoboGenius Pro C5
P. 34

    STEP - 10   Select BBC Micro:bit and click on Connect button. The Micro:bit is now
                                     connecting to the computer.

                       STEP - 11   Click on the Download button to upload the code inside the Micro:bit.

                      Now you can run your code directly on the device and explore how it works.

                      If you don’t have a real Micro:bit, you can use the Micro:bit simulator in MakeCode.
                      It behaves like a real Micro:bit allowing you to test your code, observe the output

                      and practice your ideas on the screen.

                      USING PINS FOR CONNECTIONS

                      The Micro:bit has gold strips along its bottom edge, called pins, which are used to

                      connect it to external components such as motors, sensors, buzzers and additional
                      LEDs. These pins allow the Micro:bit to send and receive signals and even provide
                      power to other devices. There are 25 pins on the edge connector, each designed

                      for different purposes. These connections make the Micro:bit more powerful and
                      versatile, allowing students to create real-world projects.

                      There are two types of pins on the Micro:bit large pins(0, 1, 2, 3V, GND) and small

                      pins (3 to 22).

                      Large Pins (0, 1, 2, 3V, GND)

                                               Pin-0                                    Pin-GND
                                                          Pin-1        Pin-2   Pin-3V

                                     RoboGenius Pro - V
                     32

| 29 30 31 32 33 34 35 36 37 38 39 |