Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 40 - RoboGenius Pro C7
P. 40

    Block based programming:

                        STEP - 8   Click the Code button to open the code editor.

                        STEP - 9   Click on the EDIT MODE dropdown button and select Blocks option.

                       STEP - 10   Click on the Create variable button in the Variables section and name it Distance.

                        STEP - 11   Drag and place the set Distance to block from the Variables section into the editor
                                   window.

                       STEP - 12   Drag and place the read ultrasonic distance sensor block from the Input section
                                   inside the set Distance to block and set the trigger pin to 2 and echo pin to 3.

                       STEP - 13   Drag and place the if then else block from the Control section. Place the comparison
                                   block from the Math section and set it to <. Compare Distance with 60.

                       STEP - 14   Inside the if (Distance < 60) block, drag and place from the Output section:
                                       print to serial monitor block and type The object is too close!

                                       set pin 4 to HIGH (to turn ON the Piezo buzzer).

                       STEP - 15   Inside the else block, drag and place from the Output section:

                                       print to serial monitor block and type It is safe to move forward.
                                       set pin 4 to LOW (to turn OFF the Piezo buzzer).

                       STEP - 16   Click on the Start Simulation button to test the system.

                      Text based programming:

                       STEP - 17   Click on the EDIT MODE dropdown button and select Text option. The code you
                                   created will be displayed here.

                                     RoboGenius Pro - VII
                     38

| 35 36 37 38 39 40 41 42 43 44 45 |