Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 44 - RoboGenius Pro C7
P. 44

    5.  Choose the correct sensor used in the Ultrasonic Distance Measurement System to measure
                             distance.

                                      (i)  Ultrasonic Sensor                    (ii)  Soil Moisture Sensor

                                    (iii)  Temperature Sensor                 (iv)  Light Sensor

                      B.  Write ‘T’ for true and ‘F’ for false.

                         1.   Multiple sensors can be connected to expand the system’s functions easily.

                         2.   The Input block is used to take readings from sensors or buttons.

                         3.   Tinkercad offers four programming modes that help both beginners
                             and advanced learners code easily.

                         4.   The Math block is used to display text or numbers on the Serial Monitor.

                         5.  The Arduino LilyPad is designed for wearable electronics like smart clothing.

                      C.  Fill in the blanks using the given hints:

                         1.                  supports a wide range of sensors that can be connected
                             with simple wiring.                                                               Hints
                                                                                                                Text
                         2.  In the Ultrasonic Distance Measurement System, the                                Arduino
                             emits a sound when an object is detected too close.                               Sensors
                                                                                                             Piezo Buzzer
                         3.  The                 mode in Tinkercad allows you to write full Arduino           Variables
                             code manually using the C++ language.

                         4.  In Arduino programming,                    is used to store data values
                             that can be reused later in the program.

                         5.                  provide live data that Arduino can process instantly for quick responses.

                      COMPETENCY-BASED QUESTIONS

                      1.  Karthik is programming an Arduino to control an LED based on sensor data. Which Tinkercad
                         programming mode is best for Karthik, a beginner, to start creating the program without
                         writing code?

                      2.  Sanya is programming her Arduino to turn on an LED when the soil moisture is below a certain
                         level. Which type of block should Sanya use to perform the comparison of soil moisture?

                                     RoboGenius Pro - VII
                     42

| 39 40 41 42 43 44 45 46 47 48 49 |