Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 71 - RoboGenius Pro C8
P. 71

    STEP - 7   Drag the drive forward block from the Drivetrain category and place it inside the
                                  if section.

                      STEP - 8   Drag the  turn right block  from the  Drivetrain category  and  place  it  inside  the
                                  else section.

                      STEP - 9   Click on the Start button to run the program.

                     The robot begins moving through the coral reef to collect trash. It uses its Front Distance Sensor
                     to detect objects and moves forward to pick them up. When no object is found, it turns right to
                     explore further. The Trash Collected display shows the total weight of debris gathered. The robot
                     runs on a battery and when the battery level becomes low, it automatically stops working until
                     recharged.

                     When the battery  reaches 0%, a pop-up  appears showing the total  trash collected.  It has
                     two buttons:
                        Get Certificate button is used to generate your certificate.

                                                                             Sensors, Logic and Maze Navigation
                                                                                                                        69

| 66 67 68 69 70 71 72 73 74 75 76 |