Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 46 - Robo_Genius_V1.0_flipbook_C3
P. 46

    21 st   #Technology Literacy
                                                                                                  Century   #Information Literacy
                                                                                                    Skills
                        Activity      Building a Car Window Glass
                                      Lifter Project

                      Step 1       Take out all the components from the smart circuit kit:

                                   1. Push switch                2. Switch             3. 2 jumpers
                                   4. Motor and fan              5. Battery            6. Magnetic Board

                                   7. USB Cable                  8. Battery OTG Socket

                                                Fan                        Motor                     Push switch

                                              Battery                    USB Cable               Battery OTG Socket

                                         Magnetic Board                    Switch                     2 jumpers

                      Step 2       Put both the switches opposite to each other.
                      Step 3       Connect both the switches with the 2-jumper module.

                      Step 4       Connect the motor and attach a fan on it.

                      Step 5       Connect the battery, Positive terminal of the battery to the motor
                                    and the negative terminal to the push switch.

                      Step 6       Turn the slide switch ON, motor will rotate as push switch is not

                                    pressed yet.

                      Step 7       Turn the slide switch OFF, motor will start rotating on pressing the
                                    push button.

                           44    RoboGenius (V1.0)-III

| 41 42 43 44 45 46 47 48 49 50 51 |