Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 45 - Robo_Genius_V1.0_flipbook_C4
P. 45

    Motor                            Diode                        Potentiometer

                                 Battery                         USB Cable                   Battery OTG Socket

                            Magnetic Board                          Fan

                     Step 2  Connect the fan on the motor.

                     Step 3  Attach the potentiometer to the negative terminal of the diode.

                     Step 4  Attach  motor  to  the  free  end  of  the  potentiometer  and  attach  a
                                battery.

                     Step 5   The negative terminal of the battery is connected to the motor and
                                the positive terminal to the positive terminal of the diode.

                                                                            Introduction to Electronics and Circuits  43

| 40 41 42 43 44 45 46 47 48 49 50 |