Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 24 - Robo_Genius_V1.0_flipbook_C4
P. 24

    Step 3

                                   P7 x 11     1 pc

                      Step 4

                                    TW1      6 pcs         Wheel     4 pcs

                                   SH100     1 pc

                      Complete

                      Output

                      In the basic car activity, when the battery is activated, the DC motor rotates

                      and drives the car straight ahead. The car moves forward or halts depending
                      on whether the switch is turned on or off. This shows how electric circuits,
                      motors, and mechanical movement function together to produce motion.

                           22    RoboGenius (V1.0)-IV

| 19 20 21 22 23 24 25 26 27 28 29 |