Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 66 - Robo_Genius_V1.0_flipbook_C7
P. 66

    Component Required

                          Small C x 2        Medium Plate x 1     Small Plate x 1      12T Gear x 1         Small L x 1

                            Motor x 1           C Holder x 2      Power Distribution           Remote x 1      Nut x 25
                                                                      board x 1

                          Small Bolt x 25     Motor Shaft x 1       Adapter x 1         Small Bar x 1       Data Cable x 1

                            Axel Lock x 1      60T Gear x 1          Spacer x 1        Small Shaft x 1       Hook x 1

                      Follow the Robo Crane Assembly Steps

                      Step 1  Take a medium plate as shown in the image.

                               Connect the two small “C” plates above the medium plate using
                               small bolts and nuts.
                               Place two C holders on the small “C” plate as shown in the image.

                               Place a Small “L” Plate between the C holders as shown in the image.

                                              Step 2  Take a small plate and fix it on top of the small “L” plate using small
                                                      bolts and nuts.

                      Step 3  Attach the motor to the motor shaft and secure it onto the small
                               plate using the screw provided with the motor.

                           64    RoboGenius (V1.0)-VII

| 61 62 63 64 65 66 67 68 69 70 71 |