Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 63 - Robo_Genius_V1.0_flipbook_C7
P. 63

    Motor x 2           Wheel x 2          Power Distribution       Remote x 1         Caster
                                                                     board x 1                             Wheel x 1

                            Small Bolt   Motor Shaft    Adapter x 1      Small Bar     Data Cable         Nut x 18
                               x 18          x 2                            x 2           x 1

                     Follow the Robo Soccer Assembly Steps

                     Step 1  Begin by placing two small “C” plates according to the image.

                              Take the two motors and attach the motor shafts to them. Place
                              the motors as shown in the image and tighten them with the
                              screws provided with the motors.

                                                Step 2  Take a medium plate and place it on top of the small “C” plates
                                                        and fix using four small bolts as shown in the image. Now, fix a
                                                        small plate in front of the medium plate using two small bolts, as
                                                        illustrated in the image.

                     Step 3  Position a small “L” plate as shown in the image and fix it with
                              the help of bolts and nuts.

                                                 Step 4  Connect  a  caster  strip  and  caster  wheel  using  small  bolts  as
                                                         depicted in the image.

                     Step 5  Attach two wheels to the motor shafts.

                     Step 6  Secure two small bars to the caster wheel.

                     Step 7  Connect  the  motor’s  wire  to  the  power  distribution  board.  Then,  connect  the  power
                              distribution board to the remote using a data cable. Finally, plug the adapter into the socket

                                                                          Mechanical Concepts with Mechatron Kit   61

| 58 59 60 61 62 63 64 65 66 67 68 |