Basic HTML Version

|  | Table of Contents |  | View Full Version

Page 60 - Robo_Genius_V1.0_flipbook_C7
P. 60

    Adapter x 1       Power Distribution     Remote x 1          Small Bar x 2    Data Cable x 1
                                                 board x 1

                                     Small Bolts x 13  Motor Shaft x 1      Axel Lock x 1         Nuts x 13

                      Follow the Robo Fan Assembly Steps

                      Step 1  Begin by  taking  two  small  “C”  plates  and placing  them
                               according to the image.

                                                       Step 2  Next, take a medium plate and secure it on top of the small
                                                               “C” plates using four small bolts as depicted in the image.
                                                               Proceed by taking a small “L” plate and positioning it as
                                                               shown in the image.

                      Step 3  Attach the motor shaft to the motor and place it on the small L-shaped bracket using the
                               screws provided with the motor.

                      Step 4  Take  two  small  bars  and  attach  them  to the  60T  gear  in  opposite
                               directions using nuts and bolts, as shown in the image.

                                                      Step 5  Now, attach the axle lock to the 60T gear and motor, and
                                                              tighten it with the screw so that the gear can move easily.

                           58    RoboGenius (V1.0)-VII

| 55 56 57 58 59 60 61 62 63 64 65 |